Laufendes-2026-695-621

//created by GHOZIIZG
//library GPS by mikalhart
//library oled by evaherrada 

#include <TinyGPS++.h> //https://github.com/mikalhart/TinyGPSPlus/blob/master/src/TinyGPS%2B%2B.h
#include <SoftwareSerial.h>
#include<Wire.h>
#include<Adafruit_GFX.h> //https://github.com/adafruit/Adafruit-GFX-Library
#include<Adafruit_SSD1306.h> //https://github.com/adafruit/Adafruit_SSD1306
int RXPin = 2;
int TXPin = 3; 
int GPSBaud = 9600; 
const int lebar=128;
const int tinggi=64;
const int reset=4;
Adafruit_SSD1306 GHOZIIZG(lebar,tinggi,&Wire,reset);
TinyGPSPlus gps;
SoftwareSerial gpsSerial(RXPin, TXPin);
void setup()
{
  GHOZIIZG.begin(SSD1306_SWITCHCAPVCC, 0x3c);
  GHOZIIZG.clearDisplay();
  gpsSerial.begin(GPSBaud);
}

void loop(){
  while (gpsSerial.available() > 0)
    if (gps.encode(gpsSerial.read()))
     GHOZIIZG.clearDisplay();
     GHOZIIZG.setTextSize(1);             
     GHOZIIZG.setTextColor(WHITE);
     GHOZIIZG.setCursor(0,1);      
     GHOZIIZG.print(F("latitude: "));
     GHOZIIZG.print(gps.location.lat(), 6);
     GHOZIIZG.setCursor(0,13);
     GHOZIIZG.print(F("longitude: "));
     GHOZIIZG.print(gps.location.lng(), 6);
     GHOZIIZG.setCursor(0,23);      
     GHOZIIZG.print(F("time: "));
     GHOZIIZG.setCursor(30,23);
     GHOZIIZG.print(gps.time.hour());
     GHOZIIZG.setCursor(50,23);
     GHOZIIZG.print(gps.time.minute());
     GHOZIIZG.setCursor(70,23);
     GHOZIIZG.print(gps.time.second());
     GHOZIIZG.setCursor(0,53);
     GHOZIIZG.setCursor(0,33);      
     GHOZIIZG.print(F("date: "));
     GHOZIIZG.setCursor(30,33);
     GHOZIIZG.print(gps.date.day());
     GHOZIIZG.setCursor(50,33);
     GHOZIIZG.print(gps.date.month());
     GHOZIIZG.setCursor(70,33);
     GHOZIIZG.print(gps.date.year());
     GHOZIIZG.setCursor(0,53);
     GHOZIIZG.print(F("created by GHOZIIZG"));
     GHOZIIZG.display();
      delay(10);

  if (millis() > 5000 && gps.charsProcessed() < 10)
  {
    GHOZIIZG.clearDisplay();
    GHOZIIZG.setTextSize(1);             
    GHOZIIZG.setTextColor(WHITE);
    GHOZIIZG.setCursor(0,13);      
    GHOZIIZG.print(F("No GPS detected"));
    GHOZIIZG.setCursor(0,23);      
    GHOZIIZG.print(F("check the cable and  restart the arduino"));
    GHOZIIZG.display();
    while(true);
  }
}